RDworksV8.1.44 is used for RD controller RDC6442G-B-LY series.(User can see that the series in the surface of controller case)


2019-06-10
Solved problems:

1.Reverse settings were invalid
2.Set the "if flowing" function to hide or no hide in the soft.ini
3.Layer setting:from 1% to 100%

2019-06-28
1.The window of installation is bliking
2.The repeat option for engrave is valid.

2019-08-28
1.The RDimage function is deteled
2.A bug of curve drawing is solved
3.Password can be saved into vendor parameter file
4.User can read the amount of files and remaining momery in documental interface 

2019-10-16
1.Allow you enter the engraving factor from 0% to 1000%

2020-07-09
1.The datas of scanning can be saved into RD-controller, RDWorksV8 software will reading and saving the datas of scanning when user does install RDWorksV8 in PC with connection. 

2020-08-15
1. Switch of the position of max power and min power 
2. Resolve the language problem for corel-plugin

2021-05-27
1. Limition of Vendor parameter, X-Max Acc:60000mm/s2£¬X-Max speed:2000mm/s, Y-Max Acc:10000mm/s2£¬Y-Max speed:500mm/s
2. Limition of User parameter, Max-Idle Acc:10000mm/s2£¬Max-Min Acc:10000mm/s2, Max-Max Acc:10000mm/s2, Max-x Acc = X-Max Acc, Max-y Acc = Y-Max Acc
3. Limition of Work parameter, Max Scan Speed:2000mm/s, Max Cut Speed:500mm/s